# SSD/MicroSD
ACTION=="add|change", KERNEL=="sd[a-z]", ATTR{queue/rotational}=="0", ATTR{queue/scheduler}="kyber"
# HDD
ACTION=="add|change", KERNEL=="sd[a-z]", ATTR{queue/rotational}=="1", ATTR{queue/scheduler}="kyber"
# NVME
ACTION=="add|change", KERNEL=="nvme[0-9]n1", ATTR{queue/rotational}=="0", ATTR{queue/scheduler}="kyber"
