# Welcome to BTstack

BTstack is [BlueKitchen's](http://bluekitchen-gmbh.com) implementation of the official Bluetooth stack.
It is well suited for small, resource-constraint devices
such as 8 or 16 bit embedded systems as it is highly configurable and comes with an ultra small memory footprint.

Targeting a variety of platforms is as simple as providing the necessary UART, CPU, and CLOCK implementations. BTstack is currently capable of connecting to Bluetooth-modules via: (H2) HCI USB, (H4) HCI UART + TI's eHCILL, and (H5) HCI Three-Wire UART.

On smaller embedded systems, a minimal run loop implementation allows to use BTstack without a Real Time OS (RTOS).
If a RTOS is already provided, BTstack can be integrated and run as a single thread.

On larger systems, BTstack provides a server that connects to a Bluetooth module.
Multiple applications can communicate with this server over different inter-process communication methods. As sockets are used for client/server communication, it's easy to interact via higher-level level languages, e.g. there's already a Java binding for use in desktop environments.

BTstack supports the Central and the Peripheral Role of Bluetooth 5 Low Energy specification incl. LE Secure Connections, LE Data Channels, and LE Data Length Extension. It can be configured to run as either single-mode stack or a dual-mode stack.

BTstack is free for non-commercial use. However, for commercial use, <a href="mailto:contact@bluekitchen-gmbh.com">tell us</a> a bit about your project to get a quote.

**Documentation:** [HTML](http://bluekitchen-gmbh.com/btstack/develop/), [PDF](http://bluekitchen-gmbh.com/btstack_develop.pdf)

**Discussion and Community Support:** [BTstack Google Group](http://groups.google.com/group/btstack-dev)

### Supported Protocols and Profiles

**Protocols:** L2CAP (incl. LE Data Channels), RFCOMM, SDP, BNEP, AVDTP, AVCTP, ATT, SM (incl. LE Secure Connections).

**Profiles:** GAP, IOP, HFP, HSP, SPP, PAN, A2DP, AVRCP incl. Browsing, GATT.

**Beta Stage:** HID, HOGP, PBAP.

**In Development:** BLE Mesh and more.

It has been qualified with the Bluetooth SIG (QDID 110883) for GAP, IOP, HFP, HSP, SPP, PAN, A2DP, AVRCP profiles and
GATT, SM of the Bluetooth 5 specification. For information on MFi/iAP2 support, please <a href="mailto:contact@bluekitchen-gmbh.com">contact us</a>.


## Evaluation Platforms

#### Embedded Platforms:      
Build Status               | Port | Platform
---------------------| -----| ------
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-esp32-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-esp32-develop) | [esp32](https://github.com/bluekitchen/btstack/tree/develop/port/esp32) | [Espressif ESP32](http://www.espressif.com/products/hardware/esp32/overview) 2.4 GHz Wi-Fi and Bluetooth Dual-Mode combo chip using [FreeRTOS](http://www.freertos.org)
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-ez430-rf2560-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-ez430-rf2560-develop) | [ez430-rf2560](https://github.com/bluekitchen/btstack/tree/develop/port/ez430-rf2560) | [EZ430-RF256x Bluetooth Evaluation Tool for MSP430](http://www.ti.com/tool/ez430-rf256x)
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-msp-exp430f5438-cc2564b-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-msp-exp430f5438-cc2564b-develop) | [msp-exp430f5438-cc2564b](https://github.com/bluekitchen/btstack/tree/develop/port/msp-exp430f5438-cc2564b) |[MSP430F5438 Experimenter Board for MSP430](http://www.ti.com/tool/msp-exp430f5438) with [Bluetooth CC2564 Module Evaluation Board](http://www.ti.com/tool/cc2564modnem)
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-msp430f5229lp-cc2564b-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-msp430f5229lp-cc2564b-develop)     | [msp430f5529lp-cc2564b](https://github.com/bluekitchen/btstack/tree/develop/port/msp430f5229lp-cc2564b) | [MSP-EXP430F5529LP LaunchPad](http://www.ti.com/ww/en/launchpad/launchpads-msp430-msp-exp430f5529lp.html#tabs) with [Bluetooth CC2564 Module Evaluation Board](http://www.ti.com/tool/cc2564modnem) and [EM Adapter BoosterPack](http://www.ti.com/tool/boost-ccemadapter) with additional 32768Hz quartz oscillator
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-max32630-fthr-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-max32630-fthr) | [max32630-fthr](https://github.com/bluekitchen/btstack/tree/develop/port/max32630-fthr) | [MAX32630FTHR ARM Cortex M4F Board](https://www.maximintegrated.com/en/products/digital/microcontrollers/MAX32630FTHR.html) with onboard [Panasonic PAN1326 module](https://na.industrial.panasonic.com/products/wireless-connectivity/bluetooth/multi-mode/series/pan13261316-series/CS467) containing  [TI CC2564B Bluetooth controller](http://www.ti.com/product/cc2564)
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-samv71-xplained-atwilc3000-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-samv71-xplained-atwilc3000-develop) | [samv71-xplained-atwilc3000](https://github.com/bluekitchen/btstack/tree/develop/port/samv71-xplained-atwilc3000) | [SAMV71 Ultra Xplained Ultra](http://www.atmel.com/tools/atsamv71-xult.aspx) evaluation kit with [ATWILC3000 SHIELD](http://www.microchip.com/DevelopmentTools/ProductDetails.aspx?PartNO=ATWILC3000-SHLD)
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-stm32-f103rb-nucleo-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-stm32-f103rb-nucleo-develop)       | [stm32-f103rb-nucleo](https://github.com/bluekitchen/btstack/tree/develop/port/stm32-f103rb-nucleo) | [STM32 Nucleo development board NUCLEO-F103RB](http://www.st.com/web/catalog/tools/FM116/SC959/SS1532/LN1847/PF259875) with [Bluetooth CC2564 Module Evaluation Board](http://www.ti.com/tool/cc2564modnem) and [EM Adapter BoosterPack](http://www.ti.com/tool/boost-ccemadapter) with additional 32768Hz quartz oscillator
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-stm32-f4discovery-cc2564b-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-stm32-f4discovery-cc2564b) | [stm32-f4discovery-cc2564b](https://github.com/bluekitchen/btstack/tree/develop/port/stm32-f4discovery-cc256x) | [STM32 F4 Discovery Board](http://www.st.com/en/evaluation-tools/stm32f4discovery.html) with [CC256xEM Bluetooth Adapter Kit for ST](https://store.ti.com/CC256XEM-STADAPT-CC256xEM-Bluetooth-Adapter-Kit-P45158.aspx) and [CC2564B Dual-mode Bluetooth® Controller Evaluation Module](https://store.ti.com/cc2564modnem.aspx)
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-stm32-l073rz-nucleo-em9304-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-stm32-l073rz-nucleo-em9304)  | [stm32-l073rz-nucleo-em9304](https://github.com/bluekitchen/btstack/tree/develop/port/stm32-l073rz-nucleo-em9304) | EM9304 DVK: [STM32 Nucleo development board NUCELO-L73RZ](https://www.st.com/en/evaluation-tools/nucleo-l073rz.html) with [EM9304  Bluetooth Controller](http://www.emmicroelectronic.com/products/wireless-rf/standard-protocols/em9304)
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-pic32-harmony-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-pic32-harmony-develop)                |  [pic32-harmony](https://github.com/bluekitchen/btstack/tree/develop/port/pic32-harmony)  | [Microchip's PIC32 Bluetooth Audio Development Kit](http://www.microchip.com/Developmenttools/ProductDetails.aspx?PartNO=DV320032)
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-wiced-h4-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-wiced-h4-develop)                           | [wiced-h4](https://github.com/bluekitchen/btstack/tree/develop/port/wiced-h4) | Broadcom/Cypress platforms that support the WICED SDK via H4 UART, e.g. [RedBear Duo](https://redbear.cc/product/wifi-ble/redbear-duo.html) (BCM43438 A1), [Inventek Systems ISM4334x](https://www.inventeksys.com/wifi/wifi-modules/ism4343-wmb-l151/) (BCM43438 A1), [Inventek Systems ISM4343](https://www.inventeksys.com/products-page/wifi-modules/serial-wifi/ism43341-m4g-l44-cu-embedded-serial-to-wifi-ble-nfc-module/) (BCM43340)
No build server | [wiced-h5](https://github.com/bluekitchen/btstack/tree/develop/port/wiced-h5) | Broadcom platforms that support the WICED SDK via H5 UART, see wiced-h4

#### Other Platforms:     
Status             | Port  | Platform
-------------------| ------|---------
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-posix-h4-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-posix-h4-develop) | [posix-h4](https://github.com/bluekitchen/btstack/tree/develop/port/posix-h4) | Unix-based system connected to Bluetooth module via H4 over serial port   
No build server | [posix-h4-da14581](https://github.com/bluekitchen/btstack/tree/develop/port/posix-h4-da14581) | Unix-based system connected to Dialog Semiconductor DA14581 via H4 over serial port
No build server | [posix-h4-da14585](https://github.com/bluekitchen/btstack/tree/develop/port/posix-h4-da14585) | Unix-based system connected to Dialog Semiconductor DA14585 via H4 over serial port   
No build server | [posix-h5](https://github.com/bluekitchen/btstack/tree/develop/port/posix-h5) | Unix-based system connected to Bluetooth module via H5 over serial port   
No build server | [posix-h5-bcm](https://github.com/bluekitchen/btstack/tree/develop/port/posix-h5) | Unix-based system connected to Broadcom/Cypress Bluetooth module via H5 over serial port   
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-libusb-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-libusb-develop) | [libusb](https://github.com/bluekitchen/btstack/tree/develop/port/libusb) | Unix-based system with dedicated USB Bluetooth dongle
No build server | [libusb-intel](https://github.com/bluekitchen/btstack/tree/develop/port/libusb-inttel) | Unix-based system with Intel Wireless 8260/8265 Controller
No build server | [windows-h4](https://github.com/bluekitchen/btstack/tree/develop/port/windows-h4) | Win32-based system connected to Bluetooth module via serial port   
No build server | [windows-winusb](https://github.com/bluekitchen/btstack/tree/develop/port/windows-winusb) | Win32-based system with dedicated USB Bluetooth dongle
No build server | [windows-winusb-intel](https://github.com/bluekitchen/btstack/tree/develop/port/windows-winusb-intel) | Win32-based system with Intel Wireless 8260/8265 Controller
No build server | [raspi](https://github.com/bluekitchen/btstack/tree/develop/port/raspi) | Raspberry Pi 3 or Raspberry Pi Zero W with built-in BCM4343 Bluetooth/Wifi Controller
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-daemon-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-daemon-develop)     | [daemon](https://github.com/bluekitchen/btstack/tree/develop/port/daemon) | TCP and Unix domain named socket client-server architecture supporting multiple clients
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/java-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/java-develop)                   | [java](https://github.com/bluekitchen/btstack/tree/develop/platform/daemon/binding/java) | Java wrapper for daemon
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-mtk-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-mtk-develop)           | [mtk](https://github.com/bluekitchen/btstack/tree/develop/port/mtk) | daemon for rooted Android devices, based on Mediatek MT65xx processor, Java and C client-server API
[<img src="http://buildbot.bluekitchen-gmbh.com/btstack/badges/port-ios-develop.svg">](https://buildbot.bluekitchen-gmbh.com/btstack/#/builders/port-ios-develop)           | [ios](https://github.com/bluekitchen/btstack/tree/develop/port/ios) | daemon for iOS jailbreak devices, C client-server API
No build server | [freertos](https://github.com/bluekitchen/btstack/tree/develop/platform/freertos) | [FreeRTOS](http://www.freertos.org): Run BTstack on a dedicated thread, not thread-safe.

## Supported Chipsets

Chipset                      | Type      | HCI Transport   | SCO over HCI     | BTstack folder | Comment
---------------------------- |-----------| ----------------|------------------|----------------|---------
Atmel ATWILC3000             | LE        | H4              | n.a.             | atwilc3000     | Firmware size: 60 kB
Broadcom UART                | Dual mode | H4, H5          | Probably         | bcm            | Max UART baudrate 2 mbps
Broadcom USB Dongles         | Dual mode | USB             | Yes              | bcm            |
CSR UART                     | Dual mode | H4, H5, BCSP    | No (didn't work) | csr            |
CSR USB Dongles              | Dual mode | USB             | Yes              | csr            |
Cypress CYW20704             | Dual mode | H4, H5, USB     | Probably         | bcm            |
Dialog Semiconductor DA14581, DA14585 | LE      | H4, SPI  | n.a.             | da14581        | Official HCI firmware used
Espressif ESP32              | Dual mode | VHCI            | Not yet          |                | SoC with Bluetooth and Wifi
EM 9301, 9304                | LE        | SPI             | n.a.             | em9301         | Custom HCI SPI implementation
Intel Dual Wireless 8260, 8265 | Dual mode | USB           | Probably         | intel          | Firmware size: 400 kB 
Nordic nRF                   | LE        | H4              | n.a.             |                | Requires custom HCI firmware
STM STLC2500D                | Classic   | H4              | No (didn't try)  | stlc2500d      | Custom deep sleep management not supported
Toshiba TC35661              | Dual mode | H4              | No               | tc3566         |
TI CC256x, WL183x            | Dual mode | H4, H5, eHCILL  | Yes              | cc256x         | Also WL185x, WL187x, and WL189x

[More infos on supported chipsets](https://bluekitchen-gmbh.com/btstack/develop/chipsets/)

## Source Tree Overview
Path				| Description
--------------------|---------------
chipset             | Support for individual Bluetooth chipsets
doc                 | Sources for BTstack documentation
example             | Example applications available for all ports
platform            | Support for special OSs and/or MCU architectures
port                | Complete port for a MCU + Chipset combinations
src                 | Bluetooth stack implementation
test                | Unit and PTS tests
tool                | Helper tools for BTstack
