RAM_START = 0x20000000;
RAM_LENGTH = 0x80000;
FLASH_START = 0x00000000;
FLASH_LENGTH = 0x200000;
DATA_FLASH_START = 0x08000000;
DATA_FLASH_LENGTH = 0x2000;
OPTION_SETTING_START = 0x0100A100;
OPTION_SETTING_LENGTH = 0x100;
OPTION_SETTING_S_START = 0x0100A200;
OPTION_SETTING_S_LENGTH = 0x100;
ID_CODE_START = 0x00000000;
ID_CODE_LENGTH = 0x0;
SDRAM_START = 0x80010000;
SDRAM_LENGTH = 0x0;
QSPI_FLASH_START = 0x60000000;
QSPI_FLASH_LENGTH = 0x4000000;
OSPI_DEVICE_0_START = 0x68000000;
OSPI_DEVICE_0_LENGTH = 0x8000000;
OSPI_DEVICE_1_START = 0x70000000;
OSPI_DEVICE_1_LENGTH = 0x10000000;

/* Board has bootloader */
FLASH_IMAGE_START = 0x10000;

INCLUDE fsp.ld
