<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">% !TEX root = btstack_gettingstarted.tex
\section{SDP Client API}
\label{appendix:api_sdp_client}
$ $
\begin{lstlisting}
 
/** 
 * @brief Queries the SDP service of the remote device given a service search pattern and a list of attribute IDs. The remote data is handled by the SDP parser. The SDP parser delivers attribute values and done event via a registered callback.
 */
void sdp_client_query(bd_addr_t remote, uint8_t * des_serviceSearchPattern, uint8_t * des_attributeIDList);

#ifdef HAVE_SDP_EXTRA_QUERIES
void sdp_client_service_attribute_search(bd_addr_t remote, uint32_t search_serviceRecordHandle, uint8_t * des_attributeIDList);
void sdp_client_service_search(bd_addr_t remote, uint8_t * des_serviceSearchPattern);
#endif
\end{lstlisting}
\pagebreak
</pre></body></html>